

 ============================================================
             code: HyFlux2 icore=           0
            executable:/home/critechuser/cycloneSurge/vers.dev/bin/mpi.HyFlux2.1
            source folder: /home/critechuser/cycloneSurge/vers.dev/src/HyFlux2
            compile option:  -O2      -DPARALLEL -I/usr/include/openmpi-x86_64
            version date: Thu Sep 17 17:40:49 CEST 2015
            execution date: Aug 28 10:32:43 CEST 2020
            current folder: /mnt/home2/scratch/storage/tmp/1000703_NOAA/1-9-calc
 ============================================================


 ============================================================
                    Argument list
 ============================================================

-i Calc_input_deck.txt
-w run2/work
-o run2
-hollandFile run2/hollandData.txt
-boundaryDir run6
-minDem -3000
-minDistSea 6
-maxDist 100
-dtstat 21600
-mask run2/mask.map

 ============================================================
                    Deck data
 ============================================================

 List of used variables
 No case sensitive =  T

 intime                           =  42.
 fintime                          =  69.
 tsave                            =  60.
 fanning                          =  0.015
 batgrid                          =  2
 lonmin                           =  -115.1000
 lonmax                           =  -100.2000
 latmin                           =  16.6000
 latmax                           =  32.0000
 mapfmt                           =  PCRaster
 mapext                           =  .map
 outfmt                           =  GTiff
 outext                           =  .tif
 radius                           =  6378388.
 houtmin                          =  1e-7
 voutmin                          =  1e-7


 ============================================================
                    Used parameters 
 ============================================================

ncore =       6

inpdeck =Calc_input_deck.txt
confdeck =/home/critechuser/cycloneSurge/DATA/config.txt
srtmpath =/home/critechuser/cycloneSurge/DATA/srtm30_plus-v5.0/data10x10
workdir =run2/work
outdir =run2
watchdir=run2/work/watch

radius =  6.378388E+06
longmin =  -115.100     [deg]
longmax =  -100.200     [deg]
latmin =   16.6000     [deg]
latmax =   32.0000     [deg]
nlong=     447
nlat =     462
dlong=  3.333334E-02 [deg]
dlat =  3.333334E-02 [deg]
dlong=   2.00000     [min]
dlat =   2.00000     [min]

intsrtm =       0
maxlev =       0
baseS =   2.00000    
reegularize =       0

demNode =run2/work/demNode.map
dem =run2/work/demSea.map
mask =run2/mask.map
dzdx =run2/work/dzdx.map
dzdy =run2/work/dzdy.map
bathymetry =run2/bathymetry.tif
batNode =
depth =
zsurf =run2/TIF_H_00151200.tif
noSlope =
fault =
rain =
fcor =
vx =run2/TIF_U_00151200.tif
vy =run2/TIF_V_00151200.tif
hollandFile =run2/hollandData.txt
boundary    =run2/work/boundary.txt
boundaryDir =run6
boundaryCode0 =       5
boundaryCode =       2
boundaryFac =   1.00000    
monitor     =monitor.txt
freqmon     =      10
parameters  =parameters.txt
console     =console.txt
login       =login.txt
logout      =logout.txt
place       =/home/critechuser/cycloneSurge/DATA/places.txt
watch       =run2/work/watch.txt
shore       =run2/work/shore.txt
outmaps     =zsurf      vx000      vy000      
restmaps     =zsurf      
statmaps     =tarr       dhjv       vnmax      u10max     deprmax    zwmax      tzwmax     hzwmax     wzwmax     

mapfmt       =PCRaster
mapext       =.map
outfmt       =GTiff
outext       =.tif
errprim =   1.000000E-06
epsvar =   1.000000E-12
errstep =   1.000000E-06
facstep =    2.00000    
hmin =   1.000000E-06
hlim =    100.000    
hcrit =    1.00000    
hprim =   1.000000E-06
g =    9.80600    
cdmax =    2.00000    

minDem =   -3000.00    
maxDem =    50.0000    
maxDepth =    20000.0    
maxDist =    100.000    
maxDistLand =    20.0000    
minDistLand =    5.00000    
minDistSea =    6.00000    
man =   1.500000E-02
manslope =   1.000000E-02
manReef =    0.00000    
demReef =   -10.0000    
expslope =   0.200000    
hvel0 =   1.000000E-02
hout =   1.000000E-02
harr =   5.000000E-02
wout =   1.000000E-02
man0 =   1.000000E-02
velmin =   1.000000E-03
hshore =   0.100000    

courmax =   0.250000    
fluxnum =    5.00000    
solver =        2
varjun =        0
maxdhmax =    100.000    
runUpLim =    50.0000    
varHLLE =        1
ilim =        4
limval =  -0.500000    
limCoeff =   0.500000       1.00000       2.00000      0.100000    
limZW =  -0.500000    
limV =  -0.500000    
seaLevel =    0.00000    
smallArg =   -1.00000    
smallNew =    1.00000    
dthydro =   -1.00000    
ntimeL =        1
tout =    248400.    
dtout   =    3600.00    
dtrest  =    61200.0    
dtstat  =    21600.0    
dtmin =   1.000000E-02
strans=             0
mapdeg=yes
entrfix=yes
verify=no 
check=no 
noSpot=yes
onlyDem=no 
nocase=yes
faultDem=yes
faultZsurf=yes
useMinDem=no 
debug=       0
postProc=no 
limnoise=no 
lamtrans =   1.000000E-02
stepmax =  1000000
timestart =    151200.    
tmax =    248400.    
imap =       42
hlim0 =    10.0000    
cmin =   3.131453E-03
ccrit =    3.13145    
ccrit0 =   0.990252    
cmin0 =   9.902525E-04
 ============================================================

